VOICE ALARM ENCODERS

Midian’s VAE-1 and VAE-10 voice alarm encoders can send a pre-recorded voice message and an Emergency ANI when an event occurs at a repeater site. The event could be that the site is on backup power, equipment has failed or an intrusion has been detected. For example the unit can be set-up to send a recorded message of “Radio Tower 1 backup power is on”. Emergency ANI is supported in Motorola’s MDC-1200, Kenwood’s FleetSync, Harris’ G-Star, DTMF and 5-Tone. Plug-in modules of the VAE-1 are available for Icom, Kenwood, Motorola and Vertex radios.