**Introducing the FirstVu™ HD Officer-Worn Video System**

The *FirstVu™ HD* from Digital Ally includes a small 1.75” camera and a separate, thin 2.75” x 4”recording module which may be securely mounted together or separately for more versatile body, vehicle, etc. mounting options. The full system weighs a mere 4 oz. and features a user-replaceable battery designed to outlast a full shift, wide 136° horizontal field of view, detailed 720p HD resolution (1280 x 720 pixels), a minimum of 16 hrs. recording time at the highest quality setting, enhanced low light sensitivity for night recording, up to 30 sec. pre-event recording to capture the events that transpired before pressing record, Instant Record ON from stand-by mode, easy one-button operation, date/time stamp, marks (important events during a recording), vibrating covert mode, non-proprietary AVI videos, secure USB access for downloading recordings or applying software upgrades, ruggedized and weather-resistant casing, evidence security and more. Visit www.digitalallyinc.com to learn more.